# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of vehicles**

**Publication reference:** EuropeAid/2020/418-074/404-83

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

**A. Supply of vehicles for SCRM**

1. The offered vehicle must meet the requirements of the applicable legal regulations of the Republic of Serbia.
2. The bidder must offer a new vehicle, which means that the vehicle is unused and shall be registered for the first time after delivery.
3. The bidder is obliged to perform a technical inspection and submit a registration sheet and a certificate of conformity as well as any other documentation required for vehicle registration upon delivery of vehicles.
4. The procurement of vehicles also includes the procurement of mandatory equipment for that vehicle.
5. The bidder will prove the technical characteristics of the supplied vehicle with a catalogue, prospectus or some other document in the Serbian language, which must contain proof for all requirements stated in the technical specification.
6. The bidder is required to submit a list of authorized services for the territory of the Republic of Serbia.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **Light duty truck**  **Qty: 3**  **General:**  • Vehicle Condition: Brand New  • Year of manufacture: 2020 or later  • Vehicle Type: Truck with double cab and box  • Type of engine: Diesel  • Euro norm: 6.2  • Vehicle Color: White  • Number of doors: 4 Doors  • Number of Seats: 5-Seater  • Mass: max 3300 kg  • Load capacity: min 900 kg  **Engine and Transmission:**  • Transmission: manual or automatic, 6 gears  • Wheel drive: Selective 4x2 - rear / 4x4  • No. of Cylinders/valves: 4/8  • Engine Capacity: 1900-2000 ccm  • Fuel Capacity: min 60 l  • Fuel type: Diesel  • Max. engine power: 110-130 kw  **Dimensions:**  • Wheelbase (mm): Min. 3220 mm  • Tire rims: Minimum R16, steel  • Length: max. 5300 mm  • Width with side mirrors: max 1900 mm  • Width: max 1820 mm |  |  |  |
|  | **Exterior:**  • Side mirrors, electro adjustable and heated  • Front Windshield, heated  • Lights, halogen and day lights  • Tow hook, removable  • Undercarriage - engine, gearbox and tank protection cover  • Differential – rear lock  • Tonneau cover – hard cover in vehicle color with installation and attestation.  **Car Trunk:**  • storage trunk – plastic protection cover for sides and floor  • trunk bed length – 1500 – 1600 mm  • trunk bed width - 1500 – 1600 mm  • width between wheel arches – min 1130 mm  • trunk bed height – min 500 mm  **Interior:**  • Driver seat, adjustable front-to-back and height  • Front passenger seat, adjustable front to back  • Air condition, manual or automatic  • Drivers wheel, electro servo with adjustable height  • Seat belt: Front and rear  • Air bag: Front Driver and passenger, side in front seats, side curtain airbags, |  |  |  |
|  | **Vehicles tools and accessories**:    • One standard Spare Wheel + standard tools  • Fire extinguisher S2  • Mandatory equipment for vehicles category N1 as provided by the legislation of the Republic of Serbia.  **Security and Safety:**  • Brake: Front disks, Rear drum  • \*ABS+EDB (Anti-lock Braking System + Electronic Brakeforce Distribution system)  • \*ESP (Electronic Stability Programme)  • \*TC (ASR+MSR) - traction control (anti-slip regulation + motor slip regulation)  • \*HLA - Hill Launch Assist  • \*HDS - Hill Descent Assist  • \*LKA - Lane keeping assistance  • \*CMS - Crash Management System  • Speed control – cruise control and limiter  **Media:**  Radio with USB and Bluetooth connection  Speakers – Min. 4  Controls on steering wheel – for audio and board computer. |  |  |  |
|  | **Warranty:**  Warranty minimum:  • Full warranty of 2 years/24 months/ without limitation in kilometers  • Warranty against corrosion – 12 years |  |  |  |